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MONTGOMERY COUNTY FIRE AND RESCUE SERVICE

DRIVER/OPERATOR TRAINING PROGRAM

Safe Driver Behavior Evaluation 
                Driver: ______________________________     Date: ___________________


    Evaluator: ______________________________________________________

 
    Unit Type& #: _______________  Emergency  _____Non-Emergency_______
Rating Values:     1=Unsatisfactory      2= Needs Improvement    3= Acceptable      

Starting   
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1. Circle Check: Completed prior to moving vehicle.


2. Mirrors and Seat:  Checked and adjusted


3. Visual Scan:  Completed before departure.


4. Seat belts: All personnel are seated and restrained.  

5. Headlights: Vehicle headlights on at all times to improve

your visibility.

In-Motion
6. Space cushion maintained: Safe following distance, 

4 second minimum to 40 MPH + 1 second per additional 10 MPH. 

7. Safe Speed:  Speed reduced for road and weather conditions, 

school zones, stopped bus, pedestrians, residential area,

parking lots, tunnel, narrow roads, overhead hazards, 

and other hazards.


8. Two hands on steering wheel:  9 and 3 hand placement

9. Shuffle Steering. Shuffle steering used appropriately, 

no palming the wheel or 1-handed turns. 

10. Turn signal: Used and flashed 2-3 times before lane change

11.      Visual Lead Time: Aim high and try to see 12-15 seconds

 ahead of you.

12.
Scan Mirrors: Scan mirrors every 6-10 seconds

               

Intersections

13.
Reduce speed:  Speed reduced to 10 MPH or less for red light,

 stop sign, using opposing lanes, or squeeze play during 

emergency response. 


14.
Intersection Stop: Vehicle completely stopped at intersection

when the intersection was not clear of moving vehicles.

15.
Visual Scan: Visual scan completed while entering 

and traversing an intersection. (Left-Right-Left)

16.
Railroad Crossing: Stopped vehicle at Railroad crossing, activated 

4-way flashers, window down & scanned before crossing. 
17.
Covered the Brake: Operator covered the brake to reduce 

reaction time while proceeding through intersection, squeeze plays, 
and other hazardous driving situations.

Arriving at Scene
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18.
Deceleration: Vehicle stopped smoothly avoiding a hard-brake.

19.
Positioning: Appropriate apparatus position, did not pass the address 
and avoided the need to back-up. 

20.
Parking Brake: Operator sets parking brake before personnel


dismount.


21.
Wheel Chock: Wheel chock properly positioned when vehicle







was parked.

Backing
22.
Avoidance: Positioned vehicle to avoid backing, and




avoided backing while turning.


23.
Positioning:  Backed unit upon arrival if appropriate.




24.
Eye contact: Maintained eye contact with spotter, and



stopped vehicle if eye contact was lost.
25.
Spotter: Positioned at left rear.






26.
Mirrors: Scanned opposite mirror every 8-10 seconds,

low speed and covered the brake.






27.
Communication: Hand signals used and understood,




drivers window rolled down.
Scene Operations

28.
Equipment: Driver set-up and operated equipment as required.

29.
Operator tasks: Driver performed required operator tasks successfully.

(Pump operations, aerial operations or Rescue Squad operations) 
30. Return to service: Driver checked equipment used and unit 

was returned to service properly.
Comments:
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